Spectrum Camera Solutions D101-X-M3068-BD Explosion-Proof 360° Camera
Certified (cFMus, ATEX, IECEx, INMETRO) for use in potentially combustible environments,this network camera can deliver 360° panoramic overviews as well as a variety of de-warped views. It supports day/night functionality for improved sensitivity in poor light. And, advanced WDR imaging technology provides clarity when there's both dark and light areas in the scene. Furthermore, it features reduced bandwidth and storage needs technology and a powerful capacity for analytics. This product is delivered factory focused and features digital roll functionality for easy installation. Made from environmentally-friendly materials, it’s re-paintable to blend in with any surroundings and there’s black, vandal-resistant and smoke-detector casings available as accessories.
• 360° panoramic view
• Advanced low-light technology and WDR imaging
• Small and discreet design
• Reduced bandwidth and storage needs technology supporting H.264 and H.265
• Environmentally friendly materials
• Temperature Range: 0°C to +40°C
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA*, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a five years manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L

Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = 0°C to +40°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta 0°C to +40°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = 0°C to +40°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = 0°C to +40°C, IP66/67
II 2 D Ex tb IIIC T85 °C Db Ta = 0°C to +40°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = 0°C to +40°C, IP66/67
Ex tb IIIC T85 °C Db Ta = 0°C to +40°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = 0°C to +40°C, IP66/67
Ex tb IIIC Db T85 °C Ta = 0°C to +40°C, IP66/67
Certificate number: NCC 20.0083 X
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class B, EN 55035, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A and B, ICES-3(A)/NMB-3(A), VCCI Class B, RCM AS/NZS CISPR 32 Class B, KC KN32 Class B, KC KN35
Safety
IEC/EN/UL 62368-1, IS 13252 
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Network
NIST SP500-267
Image sensor
12 MP (4000x3000) 1/1.7” progressive scan RGB CMOS
Lens
1.65 mm, F2.8
Horizontal field of view: 185°
Vertical field of view: 185°
Fixed iris, IR corrected
Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.32 lux at 50 IRE, F2.8
B/W: 0.06 lux at 50 IRE, F2.8
Shutter speed
1/22000 s to 1s with 50 Hz
Camera angle adjustment
Digital roll: 0–360°
System on Chip model
Manufacturer’s own chipset
Memory
2 GB RAM, 512 MB Flash
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
Overview: 2880x2880 to 160x160 (1:1)
Panorama: 3840x2160 to 192x72 (8:3, 16:9 or 32:9)
Double panorama: 3584x2688 to 384x288 (4:3 or 16:9)
Quad view: 3584x2688 to 384x288 (4:3 or 16:9)
View area 1-4: 2048x1536 to 256x144 (4:3 or 16:9)
Corner left/right: 3200x1600 to 192x72 (2:1 or 8:3)
Double corner: 2880x2880 to 384x288 (1:1 or 4:3)
Corridor: 2560x1920 to 256x144 (4:3 or 16:9)
Frame rate
360° overview only, up to 2880x2880 without WDR: 25/30 fps @ 50/60 Hz
360° overview and 4 dewarped views with WDR: up to 12.5/15 fps @ 50/60 Hz
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Multi-view streaming
360° overview, dewarped panorama, corridor, corner left/right and quad views. Up to 4 individually cropped out and dewarped view areas. All different views can be streamed simultaneously. When streaming 4 dewarped view areas and one 360° overview in max resolution: up to 14 fps per stream
Image settings
Compression, color saturation, brightness, sharpness, contrast, local contrast, white balance, day/night threshold, tone mapping, exposure control (including automatic gain control), exposure zones, advanced WDR imaging technology: up to 120 dB depending on scene, fine tuning of low-light behavior, dynamic text and image overlay, mirroring, digital roll, polygon privacy masks
Pan/Tilt/Zoom
Digital PTZ of view areas, digital PT of panorama, corner, corridor and quad views, preset positions, guard tour
Audio input/output
Two-way audio connectivity via the optional audio and I/O interfaces with portcast technology
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Event conditions
Analytics, edge storage events, virtual inputs through API
MQTT subscribe
Event actions
Record video: SD card and network share
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS, network share and email 
Pre- and post-alarm video or image buffering for recording or upload 
Notification: email, HTTP, HTTPS, TCP and SNMP trap 
PTZ: PTZ preset, start/stop guard tour 
Overlay text
MQTT publish
Data streaming
Event data

Built-in installation aids
Pixel counter, digital roll, repositioning of quad views, digital PTZ of view areas, digital PT of panorama, corner, corridor and quad views
Applications
Included
motion guard, fence guard, and loitering guard, 
video motion detection, Active tampering alarm
Supported
occupancy estimator, queue monitor, people counter, tailgating detector, direction detector, random selector
Support for enabling installation of third-party applications
Sustainability
71% recycled plastics, PVC free, BFR/CFR free (except image sensor)
Power
Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 1 Class 2
 Typical 3.7 W, max 6.49 W 
Connectors
Shielded RJ45 10BASE-T/100BASE-TX
Storage
Support for microSD/microSDHC/microSDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Recording to network-attached storage (NAS)
Operating conditions
0°C to +40°C
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)
Dimensions
Height: 292mm (11.5 in)
ø 218mm (8.6 in)

Weight
A = 19lbs (8.61kg)
S = 47lbs (21.31kg)
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese