Spectrum Camera Solutions D101-X-P3807-BD Explosion-proof PTZ Camera
Certified (cFMus, ATEX, IECEx, INMETRO) for use in potentially combustible environments, this product is a fixed dome camera with multiple sensors, providing an easy, reliable and cost-efficient one-camera installation – reducing installation time, cabling and VMS license costs. Thanks to its excellent image sensors, along with advanced low-light technology and advanced WDR imaging, it provides great video quality in any light conditions. Its four sensors give a seamless 180° panoramic overview, at up to 30 fps in 8.3 MP resolution. The camera is easy to install as recessed, flush, pendant, back-to-back, and comes with adjustable pre-set camera positions.
• Seamlessly stitched images
• 180° horizontal and 90° vertical coverage
• 8.3 MP resolution at full frame rate
• Advanced low-light technology and advanced WDR imaging
• Reduced bandwidth and storage needs technology 
• Temperature Range: -20°C to +55°C
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA*, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a five years manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L
Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = -20°C to +55°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta -20°C to +55°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
II 2 D Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC Db T85 °C Ta = -20°C to +55°C, IP66/67
Certificate number: NCC 20.0083 X
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 50121-4, IEC 62236-4, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A, KC KN32 Class A, KC KN35
Safety
IEC/EN/UL 60950-22, IEC/EN/UL 62368-1, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC/EN 60529 IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9)
Network
NIST SP500-267

Image sensor
4 x 1/2.9” progressive scan RGB CMOS 
Lens
Fixed 3.2 mm, F2.0
Horizontal field of view: 180°
Vertical field of view: 90°
M12 mount
Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.17 lux, F2.0
B/W: 0.05 lux, F2.0
Shutter speed
1/33500 to 1/10 s 
Camera angle adjustment
Pan ±180°
Tilt 0°, 35°, 45°, 55°
Roll ±5°
Model
Manufacturer’s own chipset
Memory
1024 MB RAM, 512 MB Flash
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
Motion JPEG
Resolution
4320x1920 to 480x270
Frame rate
8.3 MP (client dewarp): up to 25/30 fps (50/60 Hz) without WDR, up to 12.5/15 fps (50/60 Hz) with WDR
7.5 MP (dewarped): up to 12.5/15 fps (50/60 Hz)
Video streaming
8.3 MP (client dewarp): 1 individually configurable stream in H.264 and Motion JPEG
7.5 MP (dewarped): 2 individually configurable streams in H.264 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264
Image settings
Saturation, contrast, brightness, sharpness, advanced WDR imaging technology: up to 120 dB depending on scene, white balance, day/night threshold, exposure mode, compression, dynamic text and image overlay, exposure control, noise reduction, fine tuning of behavior at low light, polygon privacy masks
Audio input/output
Two-way audio connectivity via audio and I/O interfaces with portcast technology
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, SSL/TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Event triggers
Analytics, edge storage events, shock detection
MQTT subscribe
Event actions
Day/night mode, overlay text, video recording to edge storage, pre- and post-alarm video buffering, send SNMP trap
File upload: FTP, SFTP, HTTP, HTTPS network share, email
Notification: email, HTTP, HTTPS TCP
MQTT publish
Data streaming
Event data
Built-in installation aids
Pixel counter, leveling guide
Applications
Included
motion guard, fence guard, loitering guard, video motion detection, active tampering alarm
Support for enabling installation of third-party applications 
Sustainability
PVC free
Power
Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 1 Class 3, typical 7 W, max 12.9 W
Connectors
Shielded RJ45 10BASE-T/100BASE-TX/1000BASE-T PoE
Audio and I/O connectivity via audio and I/O interfaces with portcast technology
Storage
Support for microSD/microSDHC/microSDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Support for recording to network-attached storage (NAS)
Operating conditions
-20°C to +55°C

Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Dimensions
Height: 292mm (11.5 in)
ø 218mm (8.6 in)

Weight
A = 19lbs (8.61kg)
S = 47lbs (21.31kg)

Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese