Spectrum Camera Solutions D101-X-Q3819-BD explosion-proof Camera
Certified (cFMus, ATEX, IECEx, INMETRO) for use in potentially combustible environments, this camera delivers a 180º panoramic overview of extensive areas with high-quality images and incredible details up to 30 fps. With 14 MP resolution and seamless stitching of all four images, it offers 180° horizontal and 38° vertical coverage with no blind spots. Including a variety of mounting options, it’s also possible to mount two cameras back-to-back for a complete 360° overview. Featuring edge-to-edge technology, it’s easy to add support for audio. Additionally, a cryptographic compute module protects your camera’s device ID and simplifies authorization of the manufacturer’s devices on your network.
• 14 MP multisensor camera with one IP address
• 180° horizontal, 38° vertical coverage
• Seamlessly stitched images
• Support for audio
• Cryptographic compute module and TPM module
• Temperature Range: -20°C to +50°C
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA*, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.
The main unit shall be backed by a five years manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L
Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = -20°C to +50°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta -20°C to +50°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
II 2 D Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC Db T85 °C Ta = -20°C to +50°C, IP66/67
Certificate number: NCC 20.0083 X
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EAC, EN 55032 Class A, EN 55035, EN 50121-4, IEC 62236-4, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-3(A)/NMB-3(A), VCCI Class A, RCM AS/NZS CISPR 32 Class A, KC KN32 Class A, KC KN35, CISPR 24, CISPR 35
Safety
IEC/EN/UL 60950-22, IEC/EN/UL 62368-1, CAN/CSA C22.2 No. 62368-1, CAN/CSA-C22.2 No. 60950-22, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC/EN 60529 IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9), MIL-STD-810H (Method 501.7, 502.7, 505.7, 506.6, 507.6, 509.7, 512.6)
Network
NIST SP500-267

Image sensor
4 x 5 MP 1/2.5” progressive scan RGB CMOS 
Lens
Fixed 5.9 mm, F1.88
Horizontal field of view: 180°
Vertical field of view: 38°
Day and night
Automatically removable infrared-cut filter
Minimum illumination
With advanced WDR imaging technology and low-light technology:
Color: 0.16 lux, F2.0
B/W: 0.06 lux, F2.0
Shutter speed
1/40000 to 1/25 s 
Camera angle adjustment
Pan ± 135°
Tilt 15° to 92°
Roll ± 8°
System on Chip model
Manufacturer’s own chipset (x2)
Memory
2048 MB RAM, 512 MB Flash
Compute capabilities
Machine learning processing unit (MLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
8192x1728 (14.2 MP) to 608x128
Frame rate
14.2 MP @ 25/30 fps (50/60 Hz) WDR
Video streaming
One configurable stream in H.264, H.265 and Motion JPEG in full frame rate
Multiple individually configurable streams in reduced frame rate
Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Image settings
Saturation, contrast, brightness, sharpness, advanced WDR imaging technology: up to 120 dB depending on scene, white balance, day/night threshold, exposure mode, compression, dynamic text and image overlay, orientation aid, exposure control, noise reduction, fine tuning of behavior at low light, polygon privacy masks
Audio streaming
Two-way audio via edge-to-edge technology
Audio input/output
External microphone input, ring-power, digital audio input, automatic gain control, network speaker pairing
Audio encoding
24bit LPCM, AAC-LC 8/16/32/48 kHz, G.711 PCM 8 kHz, G.726 ADPCM 8 kHz, Opus 8/16/48 kHz, 44.1 kHz ACC-LC, LPCM
Configurable bit rate
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, protection of cryptographic keys with FIPS 140-2 certified TPM 2.0 module, cryptographic compute module with device ID
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, TCP, UDP, IGMP, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, LLDP, CDP, MQTT, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration
ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S and ONVIF® Profile T, specification at onvif.org
Event conditions
Analytics, external input, supervised external input, edge storage events, virtual inputs through API
Audio: audio detection
Digital audio: digital signal contains metadata, digital signal as invalid sample rate, digital signal missing, digital signal ok
Device status: above operating temperature, above or below operating temperature, below operating temperature, fan failure, IP address removed, network lost, new IP address, shock detected, storage failure, system ready, within operating temperature, casing open, ring power overcurrent protection
Edge storage: recording ongoing, storage disruption, storage health issues detected
I/O: digital input, manual trigger, virtual input
MQTT subscribe
Scheduled and recurring: scheduled event
Video: live stream open, average bitrate degradation, day-night mode, tampering
Event actions
Day/night mode, overlay text, video recording to edge storage, pre- and post-alarm video buffering, send SNMP trap, play audio clipm I/O events, status LED events
File upload: FTP, SFTP, HTTP, HTTPS network share, email
MQTT publish
Notification: email, HTTP, HTTPS TCP
Data streaming
Event data
Built-in installation aids
Remote Pan/tilt/roll: designed to withstand at least 200 full cycles, autoroll, pixel counter, leveling guide
Object Analytics
Object classes: humans, vehicles
Trigger conditions: line crossing, object in area
Up to 10 scenarios
Metadata visualized with color-coded bounding boxes
Polygon include/exclude areas
Perspective configuration
ONVIF Motion Alarm event
Applications
Included
object analytics
video motion detection, active tampering alarm, audio detection
Supported
Support for enabling installation of third-party applications
Sustainability
PVC free
Power
Power over Ethernet (PoE) IEEE 802.3at Type 2 Class 4
Typical 12 W, max 22.5 W
Connectors
Shielded RJ45 1000BASE-T
Terminal block for two configurable supervised inputs/digital outputs (12 V DC output, max load 50 mA), 3.5 mm analog/digital mic/line in
Storage
Support for microSD/microSDHC/microSDXC card
Support for SD card encryption
Support for recording to network-attached storage (NAS)
Operating conditions
-20°C to +50°C 
Storage conditions
-40 °C to +65°C
Humidity 5–95% RH (non-condensing)
Dimensions
Height: 292mm (11.5 in)
ø 218mm (8.6 in)

Weight
A = 19lbs (8.61kg)
S = 47lbs (21.31kg)
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese