Spectrum Camera Solutions D201-Q6078-E-BD Explosion-proof PTZ Camera
Certified (cFMus, ATEX, IECEx, INMETRO) for use in potentially combustible environments, this explosion-proof PTZ camera offers UHD 4K with 20x optical zoom for outstanding video quality. It offers great overviews and detail with the clearest, sharpest colors. This high-performance outdoor PTZ camera comes with autotracking with click and track functionality, as well as an orientation aid for active object tracking and quick orientation. Featuring built-in cybersecurity such as signed firmware and secure boot it ensures the integrity and authenticity of the firmware. Reduced bandwidth and storage needs with H.264/ H.265 significantly reduces bandwidth and storage requirements. Furthermore, object analytics offers highly granular and nuanced object classification.
• UHD 4K with 20x optical zoom
• Outstanding images with great details
• Reduced bandwidth and storage needs with support for H.264/H.265
• Object analytics
• Built-in cybersecurity features
• Temperature Range: -20°C to +50°C
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA*, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.
The main unit shall be backed by a five years manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L

Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = -20°C to +50°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta -20°C to +50°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
II 2 D Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +50°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +50°C, IP66/67
Ex tb IIIC Db T85 °C Ta = -20°C to +50°C, IP66/67
Certificate number: NCC 20.0083 X
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 55035, EN 61000-3-2, EN 61000-3-3, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A, KCC KN32 Class A, KN35
EN 50121-4, IEC 62236-4
Safety
IEC/EN/UL 60950-1
IEC/EN/UL 60950-22, IEC/EN/UL 62368–1, IS 13252
Environment
IEC/EN 60529 IP66/IP67, NEMA TS 2 (2.2.7-2.2.9), IEC 62262 IK10, ISO 4892-2, EN 50121-4, IEC 62236-4, IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-60, IEC 60068-2-78, NEMA 250 Type 4X
Network
NIST SP500-267
Midspan: EN 60950-1, GS, UL, cUL, CE, FCC, VCCI, CB, KCC, UL-AR

Image sensor
1/2.5” progressive scan RGB CMOS
Lens
4.4–88.4 mm, F2.0-3.8
Horizontal field of view: 68.3°-4.2°
Vertical field of view: 42.1°-2.34°
Autofocus, P-iris control
Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.2 lux at 30 IRE, F2.0
B/W: 0.002 lux at 30 IRE, F2.0
Shutter speed
1/10000 s to 1 s
Pan/Tilt/Zoom
Pan: 360° endless, 0.05°–450°/s
Tilt: 220°, 0.05°–450°/s
Zoom: 20x optical, 12x digital, total 240x zoom
E-flip, 256 preset positions, tour recording (max 10, max duration 16 minutes each), guard tour (max 100), control queue, on-screen directional indicator, orientation aid PTZ, set new pan 0°, adjustable zoom speed, focus recall
System on Chip model
Manufacturer’s own chipset
Memory
2 GB RAM, 512 MB Flash
Compute capabilities
Machine learning processing unit (MLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
3840x2160 4K 2160p to 320x180
Frame rate
Up to 25/30 fps (50/60 Hz) in 4K
Up to 50/60 fps (50/60 Hz) in all other resolutions
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Image settings
Manual shutter time, compression, color, brightness, sharpness, WDR – dynamic contrast, white balance, exposure control, exposure zones, fine tuning of behavior at low light, rotation: 0°, 180°, text and image overlay, polygon privacy masks, electronic image stabilization (EIS), freeze on PTZ, defog, backlight compensation, scene profiles
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1x (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot, protection of cryptographic keys with FIPS 140-2 certified TPM 2.0 module, cryptographic compute module with device ID
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, NTCIP, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile S and ONVIF® Profile T, specification at onvif.org
Event conditions
Device status: above operating temperature, above or below operating temperature, below operating temperature, fan failure, IP address removed, network lost, new IP address, shock detected, storage failure, system ready, within operating temperature
Edge storage: recording ongoing, storage disruption
I/O: manual trigger, virtual input
MQTT subscribe
PTZ: PTZ malfunctioning, PTZ movement, PTZ preset position reached, PTZ ready
Scheduled and recurring: scheduled event
Video: live stream open
Event actions
Day/night mode, overlay text, video recording to edge storage, pre- and post-alarm video buffering, send SNMP trap
PTZ: PTZ preset, start/stop guard tour
File upload via FTP, SFTP, HTTP, HTTPS network share and email
MQTT publish
Notification via email, HTTP, HTTPS and TCP
Data streaming
Event data
Built-in installation aids
Pixel counter, leveling guide
Object Analytics
Object classes: humans, vehicles
Trigger conditions: line crossing, object in area
Up to 10 scenarios
Metadata visualized with color-coded bounding boxes
Polygon include/exclude areas
Perspective configuration
ONVIF Motion Alarm event
Applications
Included
object analytics
motion guard, fence guard, loitering guard
video motion detection, autotracking 2, active gatekeeper , OSDI Zones, Orientation Aid PTZ
Support for enabling installation of third-party applications
Metal casing (aluminum), polycarbonate (PC) clear dome, sunshield (ASA)
Sustainability
PVC free
Power
High PoE 60 W SFP midspan: 100–240 V AC, max 66.1 W
Camera consumption: typical 16 W, max 51 W
Connectors
RJ45 10BASE-T/100BASE-TX PoE, RJ45 Push-pull Connector (IP66/IP67) included
Storage
Support for SD/SDHC/SDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Support for recording to network-attached storage (NAS)
Operating conditions
-20°C to +50°C
Storage conditions
-40°C to 65°C 
Dimensions
Height: 404mm (15.9 in)
ø 218mm (8.6 in)
Weight
A = 32lbs (14 kg)
S = 68lbs (28 kg)
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese