Spectrum Camera Solutions F101-Q1615-BD Explosion-Proof Camera
Certified (NEC, ATEX, IECEx) for use in potentially combustible environments, this camera combines exceptional imaging and video performance with outstanding hardware and processing capabilities including remote zoom and focus. With up to 120 fps in HDTV 1080p, it captures excellent detailed images of fast-moving objects and people. It features advanced low-light technology and advanced WDR imaging for high-quality – color – images even when recorded in near darkness. Enhanced security features such as signed firmware and secure boot ensure the integrity and authenticity of the firmware. Furthermore, it includes a deep learning processing unit enabling unique opportunities to take advantage of tailor-made third-party applications based on deep learning.
• HDTV 1080p at up to 120 fps
• Low-light technology and advanced WDR imaging
• TPM, FIPS 140-2 level 2 certified
• Embedded deep learning processing unit
• Support for third-party deep learning applications
• Operating Temperature:
	Zone system: -50°C to +60°C 
	(USA) Class/Division system: -40°C to +60°C 
• cFMus, ATEX, IECEX, EAC, UKEX/UKCA, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a five years manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing
IP66-rated, powdercoated aluminum chassis
Casing manufactured and certified by Spectrum Camera Solutions, LLC

Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 61000-3-2, EN 61000-3-3, EN 55024, EN 55035, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-3(A)/NMB-3(A), VCCI Class A, RCM AS/NZS CISPR 32 Class A, EAC, KCC KN32 Class A, KN35
Safety
IEC/EN/UL 62368-1
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Network
NIST SP500-267
Explosion-Proof Certifications
USA:
Class I Division 1 Groups BCD T5 Ta= -40°C to 60°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -40°C to 60°C, Type 4X, IP66
Certificate: FM18US0262X
Canada:
Class I Division 1 Groups BCD T5 Ta= -50°C to 60°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -50°C to 60°C, Type 4X, IP66
Class I, Zone 1, AEx/Ex db IIB+H2 T5 Gb Ta = -50°C to 60°C, Type 4X, IP66
Zone 21, AEx/Ex tb IIIC T85°C Db Ta = -50°C to 60°C, Type 4X, IP66
Certificate: FM18CA0126X
ATEX:
II 2 G Ex db IIB+H2 T5 Gb Ta = -50°C to 60°C, IP66
II 2 D Ex tb IIIC T85°C Db Ta = -50°C to 60°C, IP66
Certificate: FM18ATEX0073X
IECEx:
Ex db IIB+H2 T5 Gb Ta = -50°C to 60°C, IP66
Ex tb IIIC T85°C Db Ta = -50°C to 60°C, IP66
Certificate: IECEx FMG 18.0029X
INMETRO:
Ex db IIB+H2 T5 Gb
Ex tb IIIC T85°C Db IP66
Ta = -50°C to 60°C
Certificate: NCC 20.0084 X
EAC:
1Ex d IIB+H2 T5 Gb X, IP66
Ex tb IIIC T85°C Db X, IP66
Ambient Temperature: -50°C ≤ Tamb. ≤ +55°C
Electrical Parameters: Up to 57V and 8.2W
Electrical Parameters: 12-24 VAC/DC 24W
Certificate: RU C-US.MЮ62.B.00000/19

Image sensor
1/2.8" Progressive scan RGB CMOS
Lens
Varifocal, IR corrected, CS-mount
2 MP (16:9):
2.8–8.5 mm, F1.2 Horizontal field of view: 116°–40°
Vertical field of view: 61°–22°
i-CS lens
Day and night
Automatically removable infrared-cut filter
Minimum illumination
HDTV 1080p 25/30 fps with advanced WDR imaging technology and low-light technology:
 Color: 0.05 lux, B/W: 0.01 lux at 50 IRE, F1.2
HDTV 1080p 50/60 fps with advanced WDR imaging technology and low-light technology:
 Color: 0.1 lux, B/W: 0.02 lux at 50 IRE, F1.2
HDTV 1080p 100/120 fps:
 Color: 0.2 lux, B/W: 0.04 lux at 50 IRE, F1.2
Shutter speed
1/125000 to 2 s
System on Chip model
Manufacturer’s own chipset
Memory
2048 MB RAM, 1024 MB Flash
Compute capabilities
Deep learning processing unit (DLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC), Main, Baseline and High Profile
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
HDTV 1080p 100/120 fps (no WDR): 1920x1080​ to 160x90 HDTV 1080p 50/60 fps (WDR):1920x1080 to 160x90 HDTV 1080p 25/30 fps (WDR): 1920x1080 to 160x90
Frame rate
Up to 100/120 fps (50/60 Hz) in 1080p (no WDR)
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Video streaming indicator
Image settings
Saturation, contrast, brightness, sharpness, advanced WDR imaging technology: Up to 120 dB depending on scene, white balance, day/night threshold, tone mapping, local contrast, exposure mode, exposure zones, defogging, electronic image stabilization, barrel distortion correction, compression, rotation: auto, 0°, 90°, 180°, 270° including corridor format, dynamic text and image overlay, polygon privacy mask, mirroring of images
Scene profiles: forensic, vivid, traffic overview
Pan/Tilt/Zoom
Digital PTZ, uploadable PTZ driver (Pelco D pre-installed)
Audio streaming
Two-way, full duplex
Audio encoding
24bit LPCM, AAC-LC 8/16/32/44.1/48 kHz, G.711 PCM 8 kHz, G.726 ADPCM 8 kHz, Opus 8/16/48 kHz
Configurable bit rate
Audio input/output
External microphone input, line input, digital input with ring power, built-in microphone (can be disabled), balanced microphone, balanced input, automatic gain control, line output
24 bit AD/DA-conversion
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1x (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot, protection of cryptographic keys with FIPS 140-2 certified TPM 2.0 module
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, TLS, QoS Layer 3 DiffServ, FTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP, SNMPv1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, SFTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S and ONVIF® Profile T, specifications at onvif.org
Onscreen controls
Electronic image stabilization
Day/night shift
Defogging
Wide dynamic range
Video streaming indicator
Event conditions
Analytics, external input, supervised external input, edge storage events, virtual inputs through API
Audio: audio detection
Device status: above operating temperature, above or below operating temperature, below operating temperature, IP address removed, network lost, new IP address, shock detection, ring power overcurrent protection, storage failure, system ready, within operating temperature
Edge storage: recording ongoing, storage disruption
I/O: digital input, manual trigger, virtual input
MQTT subscribe
PTZ: PTZ malfunctioning, PTZ movement, PTZ preset position reached, PTZ ready
Scheduled and recurring: scheduled event
Video: live stream open
Event actions
MQTT publish
Record video: SD card and network share
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS, network share and email 
Pre- and post-alarm video or image buffering for recording or upload 
Notification: email, HTTP, HTTPS, TCP and SNMP trap 
PTZ: PTZ preset, start/stop guard tour 
Overlay text, external output activation, play audio clip, zoom preset, defog mode, PTZ control
Data streaming
Event data
Built-in installation aids
Focus assistant, pixel counter, leveling assistant, camera orientation aid, traffic wizard
i-CS: Remote zoom and focus
Other lens: Remote back focus
Object Analytics
Object classes: humans, vehicles (types: cars, buses, trucks, bikes)
Trigger conditions: line crossing, object in area
Up to 10 scenarios
Metadata visualized with color-coded bounding boxes
Polygon include/exclude areas
Perspective configuration
ONVIF Motion Alarm event
Applications
Included
object analytics
video motion detection, active tampering alarm, audio detection
Support for additional applications if the device is used with compatible accessories. For more information, contact your distributor partner.
Support for enabling installation of third-party applications
Sustainability
PVC free
Free of hazardous brominated and chlorinated flame retardants (BFR/CFR free)
Power
Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 1 Class 3, max 12.95 W, typical 8.2 W
10-28 V DC, max 12.1 W, typical 8.3 W
Power redundancy
Heater: 12-24 VAC/VDC 25W
Connectors
Shielded RJ45 10BASE-T/100BASE-TX/1000BASE-T PoE
DC input
I/O: 6-pin 2.5 mm terminal block for four configurable inputs/outputs(12 V DC output, max load 50 mA). Two of the ports can be supervised.
RS485/RS422, 2 pcs, 2 pos, full duplex, terminal block
3.5 mm mic/line in, 3.5 mm line out
i-CS connector (compatible with P-Iris and DC-iris)
manufacturer’s supported connector
Storage
Support for microSD/microSDHC/microSDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Recording to network-attached storage (NAS)
Operating conditions
-50°C to +60°C
US Class/Division system: -40°C to +60°C
Humidity 10-100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)
Dimensions
13.85 x 7.20 x 5.97 in (352 x 183 x 152 mm)
Weight
14 lb (6.2 kg)
Optional lenses
Lens CS 4-10 mm F0.9 P-Iris
Ricom 2MP Lens DC-iris 8-26 mm F0.9
Fujinon Varifocal Lens 8-80 mm, DC-iris
Lens i-CS 9-50 mm F1.5 8 MP
Lens CS 12-50 mm F1.4 P-Iris 8 MP
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese
Export control
The product contains U.S.-origin controlled technology/component, the US Export Administration Regulations (EAR) are always applicable to the product. You should comply at all times with all applicable national and international (re-) export control regulations.