Spectrum Camera Solutions F101-Q1715-BD Explosion-Proof Camera
Certified (NEC, ATEX, IECEx) for use in potentially combustible environments, this block camera delivers HDTV 1080p at 60 fps and 21x optical zoom for all the details. With a deep learning processing unit, it’s possible to take advantage of intelligent tailor-made applications based on deep learning on the edge. It comes with object analytics for highly nuanced object classification and reliable detection with fewer false positives. And, it provides analytics metadata based on deep learning on the edge. Lightweight in design, it’s easy to install in accessory housings and casings. It offers support for 2-way audio and supervised I/O. Furthermore, it features built-in cybersecurity features to prevent unauthorized access and safeguard your system.
• 1080p at 60 fps with 21x zoom
• Support for analytics with deep learning
• Granular object classification
• HDMI and HD-SDI output
• Operating Temperature:
	Zone system: -50°C to +50°C 
	(USA) Class/Division system: -40°C to +50°C 
• cFMus, ATEX, IECEX, EAC, UKEX/UKCA, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a five years manufacturer warranty.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing
IP66-rated, powdercoated aluminum chassis
Casing manufactured and certified by Spectrum Camera Solutions, LLC

Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55035, EN 55032 Class A, EN 61000-3-2, EN 61000-3-3, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-3(A)/NMB-3(A), KS C 9832 Class A, KS C 9835, RCM AS/NZS CISPR 32 Class A, VCCI Class A
Safety
CAN/CSA C22.2 No. 62368-1, IEC/EN/UL 62368-1
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Network
NIST SP500-267
Explosion-Proof Certifications
USA:
Class I Division 1 Groups BCD T5 Ta= -40°C to 50°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -40°C to 50°C, Type 4X, IP66
Certificate: FM18US0262X
Canada:
Class I Division 1 Groups BCD T5 Ta= -50°C to 50°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -50°C to 50°C, Type 4X, IP66
Class I, Zone 1, AEx/Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, Type 4X, IP66
Zone 21, AEx/Ex tb IIIC T85°C Db Ta = -50°C to 50°C, Type 4X, IP66
Certificate: FM18CA0126X
ATEX:
II 2 G Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, IP66
II 2 D Ex tb IIIC T85°C Db Ta = -50°C to 50°C, IP66
Certificate: FM18ATEX0073X
IECEx:
Ex db IIB+H2 T5 Gb Ta = -50°C to 50°C, IP66
Ex tb IIIC T85°C Db Ta = -50°C to 50°C, IP66
Certificate: IECEx FMG 18.0029X
INMETRO:
Ex db IIB+H2 T5 Gb
Ex tb IIIC T85°C Db IP66
Ta = -50°C to 50°C
Certificate: NCC 20.0084 X
EAC:
1Ex d IIB+H2 T5 Gb X, IP66
Ex tb IIIC T85°C Db X, IP66
Ambient Temperature Range: -50°C ≤ Tab. ≤ +50°C
Electrical Parameters: 57VDC and 13.5 W
Electrical Parameters: 12-24 VAC/VDC 20W
Certificate: RU C-US.MЮ62.B.00000/19 
Image sensor
1/2.8” progressive scan RGB CMOS 
Lens
Varifocal, 4-84.6 mm, F1.6-F4.5
Horizontal field of view: 76°–3.6°
Vertical field of view: 42°–2.2°
Autofocus, P-Iris control
Day and night
Automatically removable infrared-cut filter
Minimum illumination
1080p 25/30 fps with advanced WDR imaging technology and Advanced low-light technology:
Color: 0.1 lux at 50 IRE F1.5
B/W: 0.02 lux at 50 IRE F1.5
1080p 50/60 fps with advanced WDR imaging technology and Advanced low-light technology:
Color: 0.2 lux at 50 IRE F1.5
B/W: 0.04 lux at 50 IRE F1.5
Shutter speed
1/66500 s to 2 s 
Pan/Tilt/Zoom
Zoom: 21x optical
100 preset positions, control queue, adjustable zoom speed
System on Chip model
Manufacturer’s own chipset
Memory
2048 MB RAM, 1024 MB Flash
Compute capabilities
Deep learning processing unit (DLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
1920x1080 HDTV 1080p to 160x90
Frame rate
Up to 60/50 fps (60/50 Hz) in all resolutions
HDMI and HD-SDI are limited to 30 fps in 1080p
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG

Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Video streaming indicator
Image settings
Saturation, contrast, brightness, sharpness, advanced WDR imaging technology: up to 120 dB depending on scene, white balance, day/night threshold, tone mapping, local contrast, EIS, exposure mode, exposure zones, defogging, compression, rotation: auto, 0°, 90°, 180°, 270° including corridor format, dynamic text and image overlays, polygon privacy mask, mirroring of images Scene profiles: forensic, vivid, traffic overview
Pan/Tilt/Zoom
Uploadable PTZ driver
Audio encoding
SDI: AES3 24 bit, 48 kHz
HDMI: LPCM 24 bit, 48 kHz
Network: AAC-LC 8/16/32/44.1/48 kHz, G.711 PCM 8 kHz, G.726 ADPCM 8 kHz, Opus 8/16/48 kHz, LPCM 48 kHz
Audio input/output
External microphone input or line input, ring power, network speaker pairing
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1x (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot, cryptographic compute module, Manufacturer's device ID, secure keystore (CC EAL4 certified), TPM (FIPS 140-2 certified)
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTPS, HTTP/2, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, DHCPv4/v6, SOCKS, SSH, SIP, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Support for Session Initiation Protocol (SIP) for integration with Voice over IP (VoIP) systems, peer to peer or integrated with SIP/PBX.
Event conditions
Audio: audio clip playing, audio detection
Device status: above operating temperature, above or below operating temperature, below operating temperature, IP address removed, network lost, new IP address, ring power overcurrent protection, storage failure, system ready, within operating temperature, shock detection
Digital audio: digital signal contains metadata, digital signal has invalid sample rate, digital signal missing, digital signal OK
Edge storage: recording ongoing, storage disruption
I/O: digital input, manual trigger, virtual input
MQTT subscribe
PTZ: PTZ malfunctioning, PTZ movement, PTZ preset position reached, PTZ ready
Scheduled and recurring: scheduled event
Video: average bitrate degradation, day-night mode, live stream open, tampering
Event actions
Record video: SD card and network share
MQTT publish
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS, network share and email
Pre- and post-alarm video or image buffering for recording or upload
Notification: email, HTTP, HTTPS, TCP and SNMP trap
PTZ: PTZ preset, start/stop guard tour
Overlay text, external output activation, play audio clip, zoom preset, day/night mode , make call
Data streaming
Event data
Built-in installation aids
Leveling guide, pixel counter, license plate capture assistant
Object Analytics
Object classes: humans, vehicles (types: cars, buses, trucks, bikes)
Trigger conditions: line crossing, object in area
Up to 10 scenarios
Metadata visualized with color-coded bounding boxes
Polygon include/exclude areas
Perspective configuration
ONVIF Motion Alarm event
Applications
Included
object analytics
video motion detection
Supported
Audio Spectrum Visualizer
Support for enabling installation of third-party applications
Sustainability
PVC free
Free of hazardous brominated and chlorinated flame retardants (BFR/CFR free)
Power
Power over Ethernet (PoE) IEEE 802.3at Type 2 Class 4
10–28 V DC, typical 12 W, max 13.5 W
Heater: 12-24 VAC/VDC, 20W
Connectors
Shielded RJ45 10BASE-T/100BASE-TX/1000BASE-T PoE
I/O: 6-pin 2.5 mm terminal block for four configurable inputs
RS485/RS422, 2 pcs, 2 pos, full duplex, terminal block
3.5 mm mic/line in, 3.5 mm line out
DC input
HDMI Type A, BNC for SDI
Storage
Support for microSD/microSDHC/microSDXC card Support for SD card encryption (AES-XTS-Plain64 256bit)
Recording to network-attached storage (NAS)
Operating conditions
-50°C to +50°C
US Class/Division system: -40°C to +50°C
Humidity 10–100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)
Dimensions
13.85 x 7.20 x 5.97 in (352 x 183 x 152 mm)
Weight
14 lb (6.2 kg)

Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Polish, Traditional Chinese