Spectrum Camera Solutions D401-X-P5655-E-BD Explosion-proof PTZ Network Camera
Certified (cFMus, ATEX, IECEx, INMETRO) for use in potentially combustible environments, this product is a cost-effective, high performance explosion-proof PTZ with HDTV 1080p and 32x optical zoom. It features advanced WDR imaging technology for clarity even when there’s both dark and light areas in the scene. Advanced low-light technology to captures low-light images with more saturated colors and sharper images of moving objects. It offers electronic image stabilization and enhanced security features including signed firmware and secure boot. 
• HDTV 1080p with 32x optical zoom
• Advanced low-light technology and advanced WDR imaging
• Signed firmware and secure boot
• Focus recall and EIS
• Reduced bandwidth and storage needs technology with support for H.264 and H.265
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA*, PESO* Pending
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Temperature range: -20°C to +55°C 
• Made in Houston, Texas.

The main unit shall be backed by a five years manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third party organization, as proof of the knowledge.
Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L

Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = -20°C to +50°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta -20°C to +55°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
II 2 D Ex tb IIIC T85°C Db Ta = -20°C to +55°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC T85°C Db Ta = -20°C to +55°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC Db T85 °C Ta = -20°C to +55°C, IP66/67
Certificate number: NCC 20.0083 X
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 50121-4, IEC 62236-4, EN 61000-3-2, EN 61000-3-3, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A, KC KN32 Class A, KC KN35
Safety
IEC/EN/UL 62368-1, IEC/EN/UL 60950-22, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14,
 IEC 60068-2-27, IEC 60068-2-30, EC 60068-2-78, IEC/EN 60529
IP66, IEC/EN 62262, IK10, NEMA 250 Type 4X Network
NIST SP500-267, IPv6 USGv6
Image sensor
1/2.8” progressive scan RGB CMOS 
Lens
Varifocal, 4.3-137.6 mm, F1.4 - 4.0
Horizontal field of view: 58.3°- 2.4°
Vertical field of view: 35.5°- 1.4°
Including EIS, barrel and pincushion distortion correction
Autofocus and auto-iris
Day and night
Automatically removable infrared-cut filter
Minimum illumination
Color: 0.1 lux at 30 IRE F1.4
B/W: 0.01 lux at 30 IRE F1.4
Shutter speed
1/66500 s to 2 s 
Pan/Tilt/Zoom
Pan: 360° endless, 0.1°- 350°/s
Tilt: 180°, 0.1°- 350°/s
Zoom: 32x optical, 12x digital, Total 384x zoom
256 preset positions, nadir flip, limited guard tour, control queue, on-screen directional indicator, set new pan 0°, focus window, focus recall
Model
Manufacturer’s own chipset
Memory
1024 MB RAM, 512 MB Flash
Compute capabilities
Machine learning processing unit (MLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
1920x1080 HDTV 1080p to 320x180
Frame rate
Up to 60/50 fps (60/50 Hz) in all resolutions
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG
Controllable frame rate and bandwidth

VBR/ABR/MBR H.264/H.265
Image settings
Compression, saturation, brightness, sharpness, contrast, local contrast, white balance, exposure control, exposure zones, advanced WDR imaging technology: Up to 120 dB depending on scene, defogging, day/night shift level, tone mapping, fine tuning of low-light behavior, rotation: 0°, 180°, text and image overlay, image freeze on PTZ, electronic image stabilization, scene profiles, 20 individual polygon privacy masks
Audio streaming
Two-way, full duplex
Audio encoding
24bit LPCM, AAC-LC 8/16/32/44.1/48 kHz, G.711 PCM 8 kHz, G.726 ADPCM 8 kHz, Opus 8/16/48 kHz
Configurable bit rate
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1X (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot
Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTP/2, HTTPS, SSL/TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, RTSP, RTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, NTCIP, LLDP, CDP, MQTT v3.1.1, Syslog, Link-Local address (ZeroConf)
Application Programming Interface
Open API for software integration

ONVIF® Profile G, ONVIF® Profile S, and ONVIF® Profile T, specification at onvif.org
Event conditions
Audio: Audio detection
Device status: Above operating temperature, Above or below operating temperature, Below operating temperature, Fan failure, IP address removed, Network lost, New IP address, Shock detected, Storage failure, System ready, Within operating temperature, Edge storage, Recording ongoing, Storage disruption
I/O: Digital input, Manual trigger, Virtual input
MQTT subscribe
PTZ: PTZ malfunctioning, PTZ movement: Camera 1, PTZ preset position reached: Camera 1, PTZ ready
Scheduled and recurring: Scheduled event
Video: Day-night mode, Live stream open
Event actions
Play audio clips, day-night mode, go to preset position, guard tour, I/O, upload of images or video clips via FTP, SFTP, HTTP, HTTPS, network share and email, notification to email, HTTP, HTTPS, TCP and SNMP trap, overlay text, prioritized text, record video to SD card and network share, WDR mode
MQTT publish
Data streaming
Event data
Built-in installation aids
Pixel counter
Object Analytics
Object classes: humans, vehicles
Trigger conditions: line crossing, object in area
Up to 10 scenarios
Metadata visualized with color-coded bounding boxes
Polygon include/exclude areas
Perspective configuration
ONVIF Motion Alarm event
Applications
Included
object analytics
video motion detection, audio detection, advanced gatekeeper, autotracker 2
Support for enabling installation of third-party applications
Sustainability
PVC free
Power
PoE+ midspan 1–port: 100–240 V AC, max 37 W 
IEEE 802.3at, Type 2 Class 4
Camera consumption: typical 10.5 W, max 19 W
Multiconnector: 
20–28 V DC, typical 10 W, max 18 W
20–24 V AC, typical 15.5 V A, max 26 V A
(PoE+ midspan or power supply not included)
Connectors
RJ45 10BASE-T/100BASE-TX PoE
RJ45 push-pull connector (IP66) included
I/O connector for DC or AC input, 4 configurable alarm
Inputs/outputs: mic in/line in, line out (manufacturer’s 10-pin Push-pull System Connector or manufacturer’s Multicable C I/O Audio Power 1 m/5 m, (not included))
Storage
Support for SD/SDHC/SDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Recording to network-attached storage (NAS)
Operating conditions
-20°C to +55°C 
Maximum intermittent temperature 55 °C
Humidity 10–100% RH (condensing)
Storage conditions
-40 °C to 65 °C 
Humidity 5–95% RH (non-condensing)
Dimensions
Height: 335 mm (13.2 in)
ø 218.44 mm (8.6 in)
Weight
A = 9.98 kg (28 lbs)
S = 24.95 kg (55 lbs)
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese