Spectrum Camera Solutions D101-X-P3827-BD Explosion-Proof Panoramic Camera
Certified (cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO) for use in potentially combustible environments, this product is a panoramic dome camera with multiple sensors, providing an easy, reliable and cost-efficient one-camera installation – reducing installation time, cabling and VMS license costs. Thanks to its excellent image sensors, along with advanced low-light technology and advanced WDR imaging, it provides great video quality in any light conditions. Its four sensors give a seamless 180° panoramic overview, at up to 30 fps in 7,0 MP resolution. The camera is easy to install as recessed, flush, pendant, back-to-back, and comes with adjustable pre-set camera positions.
• 180° horizontal and 90° vertical coverage
• 7,0 MP Multi-sensor camera with 1 IP address
• Advanced low-light technology and advanced WDR imaging
• Seamlessly stitched realistic images
• Horizon Straightening
• Reduced bandwidth and storage needs technology 
• Temperature Range: -20°C to +55°C, (-4°F to +131°F)
• cFMus, ATEX, IECEx, INMETRO, UKEX/UKCA and PESO approved
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The main unit shall be backed by a five-year manufacturer warranty.
The product, including all its components, shall not contain any added PVC.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third-party organization, as proof of the knowledge.
Casing (X)
A = Aluminum casing powder coated red
S = Stainless Steel casing 316L
Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6
Ta = -20°C to +55°C
Certificate: FM17US0156X
USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb Ta -20°C to +55°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X
ATEX:
II 2 G Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
II 2 D Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, IP66/67
Certificate: FM18ATEX0057X
IECEx:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, IP66/67
Certificate: FMG 18.0020X
INMETRO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC Db T85 °C Ta = -20°C to +55°C, IP66/67
Certificate number: NCC 20.0083 X
PESO:
Ex db IIB+H2 T6 Gb Ta = -20°C to +55°C, IP66/67
Ex tb IIIC T85 °C Db Ta = -20°C to +55°C, IP66/67
Certificate: FMG 18.0020X
Approval No: A/P/HQ/MH/104/7899 (P578984)
Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
EN 55032 Class A, EN 50121-4, IEC 62236-4, EN 55024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A, KC KN32 Class A, KC KN35
Safety
IEC/EN/UL 60950-22, IEC/EN/UL 62368-1, IS 13252
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC/EN 60529 IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9)
Network
NIST SP500-267

Image sensor
4 x 1/2.8” progressive scan RGB CMOS 
Lens
Fixed 3.3 mm, F2.0
Horizontal field of view: 180°
Vertical field of view: 90°
Day and night
Automatic infrared-cut filter
Hybrid infrared-cut filter
Minimum illumination
Color: 0.15 lux, F2.0
B/W: 0.05 lux, F2.0
Shutter speed
1/31500 to 1.5 secs 
Camera angle adjustment
Pan ±180°
Tilt 0° to 50°
Roll ±5°
Model
Manufacturer’s own chipset
Memory
2024 MB RAM, 8192 MB Flash
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
3712x1856 to 640x320
Frame rate
Up to 25/30 fps (50/60Hz) in all resolutions
Video streaming
Up to 20 unique and configurable video streams
AXIS Zipstream technology in H.264 and H.265
Controllable frame rate and bandwidth
VBR/ABR/MBR H.264
Low latency mode
Video Streaming 
Image settings
Horizon straightening, saturation, contrast, brightness, sharpness, white balance, day/night threshold, local contrast, tone mapping, exposure mode, compression, dynamic text and image overlay, polygon privacy masks
Audio input/output
Input – for external unbalanced microphone, optional 5V microphone power. Digital input, optional 12V ring power. Unbalanced line input.
Output – via network speaker pairing.
Security
IEEE 802.1X (EAP-TLS, PEAP-MSCHAPv2), IEEE 802.1AR, HTTPS/HSTS, TLS v1.2/v1.3, Network Time Security (NTS), X.509 Certificate PKI, IP address filtering

Supported protocols
IPv4, IPv6 USGv6, ICMPv4/ICMPv6, HTTP, HTTPS, HTTP/2, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, mDNS (Bonjour), UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS/DNSv6, DDNS, NTP, NTS, RTSP, RTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SSH, LLDP, CDP, MQTT v3.1.1, Secure syslog (RFC 3164/5424, UDP/TCP/TLS), Link-Local address (ZeroConf), IEEE 802.1X (EAP-TLS), IEEE 802.1AR IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9),
MIL-STD-810H (Method 501.7, 502.7, 505.7, 506.6, 507.6, 509.7, 512.6)
Application Programming Interface
Open API for software integration, including VAPIX®, metadata and AXIS Camera Application Platform (ACAP)
One-click cloud connection
ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T
Event triggers
Device status: above operating temperature, above or below operating temperature, below operating temperature, within operating temperature, IP address removed, new IP address, network lost, system ready, ring power overcurrent protection, live stream active, casing open
Digital audio input status
Edge storage: recording ongoing, storage disruption, storage health issues detected
I/O: digital input, manual trigger, virtual input
MQTT: subscribe
Scheduled and recurring: schedule
Video: average bitrate degradation, day-night mode, live stream, tampering
Event actions
Audio clips: play, stop
Day-night mode
I/O: toggle I/O once, toggle I/O while the rule is active
MQTT: publish
Notification: HTTP, HTTPS, TCP and email
Overlay text
Recordings: SD card and network share
SNMP traps: send, send while the rule is active
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS,
network share and email
Power
IEEE802.3at 18W Max
Operating conditions
-20°C to +55°C, (-4°F to +131°F)

Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5-95% RH (non-condensing)
Dimensions
Height: 292mm (11.5 in)
ø 218mm (8.6 in)

Weight
A = 25.6lbs (11.6kg)
S = 52.7lbs (23.9kg)

Warranty
5- year warranty, see https://www.spectrumcamera.com

Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Traditional Chinese