Spectrum D412-X-NDP-5522-Z30-BD Explosion-Proof HDTV 1080p PTZ Camera

Certified (cFMus, IECEx, ATEX, INMETRO, UKCA and PESO) for use in potentially combustible environments, this explosion-proof PTZ camera provides HDTV 1080p resolution with 30x optical zoom. Enclosed in a patented stainless-steel or red aluminum housing, it features Starlight technology for excellent low-light performance, 120dB dynamic range, and built-in Essential Video Analytics.

• HDTV 1080p with 30x optical zoom, 16x digital zoom
• Starlight camera technology with excellent low-light performance
• 120dB dynamic range (HDR)
• Built-in Essential Video Analytics
• Intelligent streaming, IDNR and H.265 reduce bit rate
• Made in USA
• NDAA-Compliant
• cFMus, Class I/II/III, Division 1, Zone 1/21, IECEX, ATEX, INMETRO, UKCA and PESO approved
• Operating Temperature: -20°C to +55°C
• 5 Year Warranty

The main unit shall be backed by a five-year manufacturer warranty.

Explosion-proof Certifications
USA (Divisions):
Class I Division 1 Groups B,C,D T6, Ta = -20°C to +55°C, Type 4X, IP66/67
Class II/III, Division 1, Groups E,F,G T6, Ta = -20°C to +55°C
Certificate: FM17US0156X

USA and Canada (Zones):
Class I, Zone 1, AEx/Ex db IIB+H2 T6 Gb, Ta = -20°C to +55°C, Type 4X, IP66/67
Zone 21, AEx/Ex tb IIIC T85°C Db, Ta = -20°C to +55°C, Type 4X, IP66/67
Certificate: FM17US0156X and FM18CA0103X

ATEX:
II 2 G Ex db IIB+H2 T6 Gb, Ta = -20°C to +55°C, IP66/67
II 2 D Ex tb IIIC T85°C Db, Ta = -20°C to +55°C, IP66/67
Certificate: FM18ATEX0057X

IECEx:
Ex db IIB+H2 T6 Gb, Ta = -20°C to +55°C, IP66/67
Ex tb IIIC T85°C Db, Ta = -20°C to +55°C, IP66/67
Certificate: FMG 18.0020X

INMETRO:
Ex db IIB+H2 T6 Gb, Ta = -20°C to +55°C, IP66/67
Ex tb IIIC Db T85°C, Ta = -20°C to +55°C, IP66/67
Certificate: NCC 20.0083 X

PESO:
Ex db IIB+H2 T6 Gb, Ta = -20°C to +55°C, IP66/67
Ex tb IIIC T85°C Db, Ta = -20°C to +55°C, IP66/67
Certificate: FMG 18.0020X

Approvals
Hazardous Area: FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, 60079-1, 60079-31
EMC: EN 55032 Class A, EN 50121-4, FCC Part 15 Subpart B Class A
Safety: IEC/EN/UL 60950-22, IEC/EN/UL 62368-1, IS 13252
Environment: IEC 60068 series, IEC/EN 60529 IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X
Network: NIST SP500-267

Camera
Image sensor: 1/2.8" CMOS
Total Sensor Pixels: 2.13MP Approx.
Sensitivity (Color): 0.0186 lux (Starlight technology)
Sensitivity (Monochrome): 0.0040 lux
Day/Night Modes: Auto, Color, Monochrome
White Balance: Basic, Standard, Dominant color, Sodium lamp auto

Pan/Tilt/Zoom
Zoom: 30x Optical, 16x Digital
Focal Length: 4.5 to 135mm
Aperture: F1.6 to 4.4
Horizontal Field of View: 2.4° to 60.9°
Tours: 2 recorded tours (15 min max), 1 pre-position tour (256 scenes)

Video
Video Compression: H.265, H.264, M-JPEG
Frame Rate: 60 fps
Resolution: 1920 x 1080 (HDTV 1080p), 1280 x 720, 640 x 480 and more
WDR Technology: HDR (120 dB)
Backlight Compensation: On/Off, Intelligent Auto Exposure (IAE)
Privacy Masks: 32

Audio
Audio input/output: Line In, Line Out
Compression: G.711, L16, AAC

Network
Conformity: ONVIF Profile S, Profile G, Profile T
Protocols: IPv4, IPv6, HTTP, HTTPS, TCP, UDP, RTSP, FTP, DHCP, SNMP

Analytics
Analysis Type: Essential Video Analytics
Alarm Triggers: Any object, Object in field, Line crossing, Enter/leave field, Loitering, Counting, Crowd density estimation, Tampering

General
Casing (Options): A = Aluminum, S = Stainless Steel
Weight (Aluminum): 29 lbs (13.2 kg)
Weight (Stainless Steel): 55 lbs (24.95 kg)
Dimensions: Height: 13.2 in (335 mm), ø 8.6 in (218 mm)
Power: PoE IEEE 802.3at (Max 25W)
Storage Conditions: -40°C to +60°C (-40°F to 140°F)
Operating Conditions: -20°C to +55°C (-4°F to 131°F)
Warranty: 5-year limited warranty