Spectrum Camera Solutions F101-Q1656-BD Explosion-Proof Camera
Certified (NEC, ATEX, IECEX, EAC, INMETRO, UKEX/UKCA and PESO) for use in potentially combustible environments, with 4 MP resolution at up to 60 fps, a 1/1.8” sensor, and advanced low-light technology, the camera delivers exceptional video quality even in poor light conditions. Based on the manufacturer’s latest own chipset, it offers support for advanced features and powerful applications based on deep learning on the edge. And object analytics offers highly nuanced object classification. This high-performance box camera includes premium functionality and support for PoE and redundant DC power. Furthermore, built-in cybersecurity features, such as cryptographic compute module, signed firmware and secure boot, and FIPS-certified TPM, prevent unauthorized access and safeguard your system.
• Exceptional images with 1/1.8” sensor
• Support for analytics with deep learning
• Built-in cybersecurity features
• Comparable to Axis 02462-001 XFQ1656 Explosion-Protected Camera
• Premium camera functionality
• Remote zoom and focus
• Operating Temperature:
	Zone system: -50°C to +60°C 
	(USA) Class/Division system: -40°C to +60°C 
• cFMus, ATEX, IECEX, EAC, INMETRO, UKEX/UKCA and PESO approved
• Class I II III Division 1 Gr B,C,D,E,F,G; II 2 G Ex db IIB+H2 Gb II 2 D Ex tb IIIC T85°C Db
• Made in Houston, Texas.

The embedded analytics shall be backed by free support within warranty period.
The main unit shall be backed by a five-year manufacturer warranty.
The contractor or designated subcontractor shall submit credentials of completed manufacturer certification, verified by a third-party organization, as proof of the knowledge.
Casing
IP66-rated, powder-coated aluminum chassis
Casing manufactured and certified by Spectrum Camera Solutions, LLC

Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31
EMC
CISPR 24, CISPR 35, EN 55032 Class A, EN 55035, EN 61000-3-2, EN 61000-3-3, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-3(B)/NMB-3(B), KS C 9832 Class A, KS C 9815, KS C 9835, KS C 9547, RCM AS/NZS CISPR 32 Class A, VCCI Class A
Safety
IEC/EN/UL 62368-1
Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 60068-2-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78
Network
NIST SP500-267
Explosion-Proof Certifications
USA:
Class I Division 1 Groups BCD T5 Ta= -40°C to 60°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -40°C to 60°C, Type 4X, IP66
Certificate: FM18US0262X
Canada:
Class I Division 1 Groups BCD T5 Ta= -50°C to 60°C, Type 4X, IP66
Class II/III Division 1 Groups EFG Ta= -50°C to 60°C, Type 4X, IP66
Class I, Zone 1, AEx/Ex db IIB+H2 T5 Gb Ta = -50°C to 60°C, Type 4X, IP66
Zone 21, AEx/Ex tb IIIC T85°C Db Ta = -50°C to 60°C, Type 4X, IP66
Certificate: FM18CA0126X
ATEX:
II 2 G Ex db IIB+H2 T5 Gb Ta = -50°C to 60°C, IP66
II 2 D Ex tb IIIC T85°C Db Ta = -50°C to 60°C, IP66
Certificate: FM18ATEX0073X
IECEx:
Ex db IIB+H2 T5 Gb Ta = -50°C to 60°C, IP66
Ex tb IIIC T85°C Db Ta = -50°C to 60°C, IP66
Certificate: IECEx FMG 18.0029X
INMETRO:
Ex db IIB+H2 T5 Gb
Ex tb IIIC T85°C Db IP66
Ta = -50°C to 60°C
Certificate: NCC 20.0084 X
PESO:
Ex db IIB+H2 T5 Gb Ta = -50°C to +60°C, IP66
Ex tb IIIC T85°C Db Ta = -50°C to +60°C, IP66
Certificate: IECEx FMG 18.0029X
Approval No: A/P/HQ/MH/104/7899 (P578984)
EAC:
1Ex d IIB+H2 T5 Gb X, IP66
Ex tb IIIC T85°C Db X, IP66
Ambient Temperature Range: -50°C ≤ Tamb ≤ +60°C
Electrical Parameters: 57VDC and 8.2W
Electrical Parameters: 12-24 VAC/VDC 25W
Certificate: RU C-US.MЮ62.B.00000/19
Image sensor
1/1.8” progressive scan RGB CMOS 
Lens
Varifocal, 3.9–10 mm, F1.5
Horizontal field of view: 120°–47°
Vertical field of view: 63°–27°
Autofocus, i-CS lens, IR corrected, remote zoom and focus, P-Iris control
Minimum focus distance: 0.5 m (1.6 ft)
Day and night
Automatically removable infrared-cut filter
Minimum illumination
4 MP 25/30 fps with advanced WDR imaging technology and low-light technology 2.0
Color: 0.05 lux at 50 IRE, F1.5
B/W: 0.01 lux at 50 IRE, F1.5
4 MP 50/60 fps with low-light technology 2.0
Color: 0.1 lux at 50 IRE, F1.5
B/W: 0.02 lux at 50 IRE, F1.5
4 MP 25/30 fps with advanced WDR imaging technology and low-light technology 2.0
With optional F0.9 lens
Color: 0.02 lux at 50 IRE, F0.9
B/W: 0.004 lux at 50 IRE, F0.9
Shutter speed
1/47500 s to 1 s
Model
Manufacturer’s own chipset
Memory
2048 MB RAM, 8194 MB Flash
Compute capabilities
Deep learning processing unit (DLPU)
Video compression
H.264 (MPEG-4 Part 10/AVC) Baseline, Main and High Profiles
H.265 (MPEG-H Part 2/HEVC) Main Profile
Motion JPEG
Resolution
16:9 2688x1512 Quad HD to 160x90
4:3 2016x1512 to 160x120
Frame rate
No WDR: Up to 60/50 fps (60/50 Hz) in all resolutions
WDR: Up to 30/25 fps (60/50 Hz) in all resolutions
Video streaming
Multiple, individually configurable streams in H.264, H.265 and Motion JPEG
Controllable frame rate and bandwidth
VBR/ABR/MBR H.264/H.265
Video streaming indicator

Multi-view streaming
Up to 8 individually cropped out view areas
Image settings
Saturation, contrast, brightness, advanced WDR imaging technology: Up to 120 dB depending on scene, white balance, day/night threshold, tone mapping, exposure mode, exposure zones, defogging, barrel distortion correction, electronic image stabilization, compression, rotation: 0°, 90°, 180°, 270° including corridor format, mirroring, dynamic text and image overlay, polygon privacy mask
Pan/Tilt/Zoom
Digital PTZ, 2.5x optical zoom, preset positions
Uploadable PTZ driver (Pelco D pre-installed)
Audio streaming
Two-way, full duplex
Noise reduction
Audio encoding
24bit LPCM, AAC-LC 8/16/32/48 kHz, G.711 PCM 8 kHz, G.726 ADPCM 8 kHz, Opus 8/16/48 kHz
Configurable bit rate
Audio input/output
External microphone input or line input, line output, built-in microphone (can be disabled), ring power, digital audio input, automatic gain control
Security
Password protection, IP address filtering, HTTPS encryption, IEEE 802.1x (EAP-TLS) network access control, digest authentication, user access log, centralized certificate management, brute force delay protection, signed firmware, secure boot, protection of cryptographic keys with FIPS 140-2 certified TPM 2.0 module, cryptographic compute module with device ID
Supported protocols
IPv4, IPv6 USGv6, HTTP, HTTPS, HTTP/2, TLS, QoS Layer 3 DiffServ, FTP, SFTP, CIFS/SMB, SMTP, Bonjour, UPnP®, SNMP v1/v2c/v3 (MIB-II), DNS, DynDNS, NTP, RTSP, RTP, SRTP, TCP, UDP, IGMPv1/v2/v3, RTCP, ICMP, DHCPv4/v6, ARP, SOCKS, SSH, LLDP, MQTT v3.1.1, Syslog
Application Programming Interface
Open API for software integration
ONVIF® Profile G, ONVIF® Profile M, ONVIF® Profile S, and ONVIF® Profile T
Onscreen controls
Electronic image stabilization
Day/night shift
Defogging
Wide dynamic range
Video streaming indicator

Event conditions
Analytics, external input, supervised external input, edge storage events, virtual inputs through API
Audio: audio detection
Device status: above operating temperature, above or below operating temperature, below operating temperature, IP address removed, network lost, new IP address, shock detected, storage failure, system ready, within operating temperature
Edge storage: recording ongoing, storage disruption
I/O: digital input, manual trigger, virtual input
PTZ: PTZ malfunctioning, PTZ movement, PTZ preset position reached, PTZ ready
Scheduled and recurring: scheduled event
Video: live stream open
Event actions
Record video: SD card and network share
Upload of images or video clips: FTP, SFTP, HTTP, HTTPS, network share and email
Pre- and post-alarm video or image buffering for recording or upload
Notification: email, HTTP, HTTPS, TCP and SNMP trap
PTZ: PTZ preset, start/stop guard tour
Overlay text, external output activation, play audio clip, zoom preset
Data streaming
Event data
Built-in installation aids
Remote zoom and focus, remote back focus, leveling assistant, pixel counter
Object Analytics
Object classes: humans, vehicles (types: cars, buses, trucks, bikes)
Trigger conditions: line crossing, object in area
Up to 10 scenarios
Metadata visualized with color-coded bounding boxes
Polygon include/exclude areas
Perspective configuration
ONVIF® Motion Alarm event
Applications
Included
object analytics
video motion detection
Supported
Support for enabling installation of third-party applications
Sustainability
PVC free
Free of hazardous brominated and chlorinated flame retardants (BFR/CFR free)
Power
Power over Ethernet (PoE) IEEE 802.3af/802.3at Type 1 Class 3
Typical 5.1 W, max 8.2 W
10–28 V DC, typical 4.6 W, max 7.7 W
Power redundancy
Heater: 12-24 VAC/VDC 25W

Connectors
RJ45 10BASE-T/100BASE-TX/1000BASE-T PoE
Terminal block for two supervised and two unsupervised configurable inputs / digital outputs (12 V DC output, max load 50 mA)
RS485/RS422, 2 pcs, 2 pos, full duplex, terminal block
DC input, terminal block, 3.5 mm mic/line in, 3.5 mm line out
i-CS connector (compatible with P-Iris and DC-iris)
manufacturer’s supported connector
Storage
Support for microSD/microSDHC/microSDXC card
Support for SD card encryption (AES-XTS-Plain64 256bit)
Recording to network-attached storage (NAS)
Operating conditions
-50°C to +60°C
US Class/Division system: -40°C to +60°C
Humidity 10–100% RH (condensing)
Storage conditions
-40 °C to 65 °C (-40 °F to 149 °F)
Humidity 5–95% RH (non-condensing)
Dimensions
13.85 x 7.20 x 5.97 in (352 x 183 x 152 mm)
Weight
14 lb (6.2 kg)
Optional lenses
Lens CS 4-10 mm F0.9 P-Iris
Lens i-CS 9-50 mm F1.5 8 MP
Lens CS 12-50 mm F1.4 P-Iris 8 MP
Languages (Camera)
English, German, French, Spanish, Italian, Russian, Simplified Chinese, Japanese, Korean, Portuguese, Polish, Traditional Chinese