Spectrum F202-BBBBB-CC-DD-EE-FF Explosion-Proof 2MP, 4MP, 6MP & 8MP (4K) Fixed Cameras

Certified (CFMus, Class I/II/III, Division 1, Groups BCDEFG, II 2 G Ex db IIB+H2 Gb, II 2 D Ex tb IIIC Db, IECEx & ATEX) for use in potentially combustible environments, this product is a fixed camera available in 2MP, 4MP, 6MP & 8MP (4K) resolutions. It features Pelco Smart Analytics, Cloud-based AI Intelligence, and multiple power and connectivity options including POE, 4G/5G, and SFP Media Converters.

• Excellent Image Quality 2MP, 4MP, 6MP & 8MP (4K)
• Pelco Smart Analytics inside
• Cloud-based AI Intelligence
• POE and Redundant DC Power
• 4G and 5G Wireless options available
• SFP Media Converter option available
• Operating Temperature: Varies by model, from -50°C to +65°C
• Made in USA
• NDAA and TAA-Compliant
• CFMus, Class I/II/III, Division 1, Groups BCDEFG
• II 2 G Ex db IIB+H2 Gb
• II 2 D Ex tb IIIC Db, IECEx & ATEX approved
• 5 Year Warranty with Registration

The main unit shall be backed by a five-year manufacturer warranty with registration.

Part No.: F202-SRXE4P-2-IBX-1-01-01
Description: POE - IEEE 802.3bt-90W
MP: 2.0
F Number: 1.4
Lens: 3.9-10mm, 1/2.8" Sensor

Part No.: F202-SRXE4P-2-IBX-1-02-02
Description: Media Converter (SFP) - 120/240 VAC 50/60 Hz
MP: 2.0
F Number: 1.4
Lens: 3.9-10mm, 1/2.8" Sensor

Part No.: F202-SRXE4P-2-IBX-1-02-03-02-RUT241
Description: Wireless Teltonika 4G - 120/240 VAC 50/60 Hz
MP: 2.0
F Number: 1.4
Lens: 3.9-10mm, 1/2.8" Sensor

Part No.: F202-SRXE4P-2-IBX-1-02-03-03-XR60
Description: Wireless Sierra 5G - 120/240 VAC 50/60 Hz
MP: 2.0
F Number: 1.4
Lens: 3.9-10mm, 1/2.8" Sensor

Part No.: F202-SRXE4P-4-IBX-1-01-01
Description: POE - IEEE 802.3bt-90W
MP: 4.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-4-IBX-1-02-02
Description: Media Converter (SFP) - 120/240 VAC 50/60 Hz
MP: 4.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-4-IBX-1-02-03-02-RUT241
Description: Wireless Teltonika 4G - 120/240 VAC 50/60 Hz
MP: 4.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-4-IBX-1-02-03-03-XR60
Description: Wireless Sierra 5G - 120/240 VAC 50/60 Hz
MP: 4.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-6-IBX-1-01-01
Description: POE - IEEE 802.3bt-90W
MP: 6.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-6-IBX-1-02-02
Description: Media Converter (SFP) - 120/240 VAC 50/60 Hz
MP: 6.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-6-IBX-1-02-03-02-RUT241
Description: Wireless Teltonika 4G - 120/240 VAC 50/60 Hz
MP: 6.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-6-IBX-1-02-03-03-XR60
Description: Wireless Sierra 5G - 120/240 VAC 50/60 Hz
MP: 6.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-8-IBX-1-01-01
Description: POE - IEEE 802.3bt-90W
MP: 8.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-8-IBX-1-02-02
Description: Media Converter (SFP) - 120/240 VAC 50/60 Hz
MP: 8.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-8-IBX-1-02-03-02-RUT241
Description: Wireless Teltonika 4G - 120/240 VAC 50/60 Hz
MP: 8.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Part No.: F202-SRXE4P-8-IBX-1-02-03-03-XR60
Description: Wireless Sierra 5G - 120/240 VAC 50/60 Hz
MP: 8.0
F Number: 1.3
Lens: 3.9-10mm, 1/1.8" Sensor

Explosion-proof Certifications
USA (Divisions): Class I Division 1 Groups BCD, Class II/III, Division 1, Groups EFG
USA and Canada (Zones): Class I, Zone 1, AEx/Ex db IIB+H2 Gb, Zone 21, AEx/Ex tb IIIC Db
ATEX: II 2 G Ex db IIB+H2 Gb, II 2 D Ex tb IIIC Db
IECEx: Ex db IIB+H2 Gb, Ex tb IIIC Db

Certificates:
USA: FM24US0209X
Canada: FM24CA0056X
ATEX: FM24ATEX0026X
IECEx: IECEX_FMG_24.0028_000

Approvals
Hazardous Area
FM3600, FM3615, ANSI/ISA/EN/IEC/CAN/CSA-C22.2 60079-0, ANSI/UL/EN/IEC/CAN/CSA-C22.2 60079-1, ANSI/UL/IEN/EC/CAN/CSA-C22.2 60079-31

EMC
EN 60032 Class A, EN 50121-4, IEC 62236-4, EN 60024, EN 61000-6-1, EN 61000-6-2, FCC Part 15 Subpart B Class A, ICES-003 Class A, VCCI Class A, RCM AS/NZS CISPR 32 Class A, KC KN32 Class A, KC KN35

Safety
IEC/EN/UL 60950-22, IEC/EN/UL 62368-1, IS 13252

Environment
IEC 60068-2-1, IEC 60068-2-2, IEC 600682-6, IEC 60068-2-14, IEC 60068-2-27, IEC 60068-2-78, IEC/EN 60529 IP66/IP67, IEC/EN 62262 IK10, NEMA 250 Type 4X, NEMA TS 2 (2.2.7-2.2.9)

Network
NIST SP500-267

General
Casing: Aluminum
Weight: 27-29 lbs (12.2-13.2 kgs)
Dimensions: 19.25(L) x 7.41(H) x 6.64(W) in (498 x 188 x 163 mm)
Power: See model selection table
Storage Conditions: -40°C to +60°C (-40°F to +140°F), Humidity 5-95% RH (non-condensing)
Operating Conditions: See specific model table (e.g., -50°C to +65°C for F202-SRXE4P-2-IBX-1-01-01)
Warranty: 5-year warranty with registration