Spectrum FEZB-H105Q 4MP 10x Explosion Proof Bullet Camera

Certified (ATEX & IECEx) for use in potentially combustible environments, this explosion-proof camera delivers 4MP resolution with a 10x optical zoom at 30fps. Enclosed in a 316L Stainless Steel housing, it is a lightweight camera designed for easy installation.

• 4MP Resolution
• 1/2.8" Sony CMOS Sensor
• 10x Optical Zoom (4.7mm to 47.0mm)
• 32x Digital Zoom
• Digital Noise Reduction (DNR)
• 316L Stainless Steel Construction
• IP67, IK10
• PoE+ Support
• H.265, H.264, MJPEG Triple Streams
• ONVIF Compatibility
• 5 Year Warranty

The main unit shall be backed by a five-year manufacturer warranty.

Explosion-proof Certifications
ATEX & IECEx
II 2 G Ex db IIC T6/T5 Gb
II 2 D Ex tb IIIC T80°C/T85°C Db
Certificate: IECEX KTL 24.0019X

Approvals
IP Rating: IP67
IK Rating: IK10

Camera
Image Sensor: 1/2.8" Sony CMOS Sensor
Active Pixels: 5.13M (2616 x 1960)
Lens: 10x Day & Night Zoom Lens
Focal Length: 4.7mm ~ 47.0mm
Zoom: 10x Optical, 32x Digital
Angle of View (Horizontal): 58.3° (Wide) to 7.1° (Tele)
Minimum illumination (Color): 0.02 lux / DSS 0.002 lux
Minimum illumination (B/W): 0.005 lux / DSS 0.0005 lux
Shutter speed: Auto (1/30~1/10,000 sec)
DNR (Digital Noise Reduction): 2D/3D, 2D+3D
WDR: ACE (D-WDR)
Defog: On/Off

Video
Video Compression: H.265, H.264, MJPEG
Resolution: 2560x1440, 1920x1080, 1280x720, 640x480, 640x360
Frame Rate (Max): 30fps at all resolutions
Video Streaming: Triple Stream

Network
Interface: RJ45 10/100 Base-T PoE
API: Onvif Profile S
Supported Protocols: TCP/IP, UDP/IP, RTP, RTSP, RTCP, NTP, HTTP, DHCP, FTP, SMTP, DNS, DDNS

General
Casing: Stainless Steel 316L
Weight: 7.72 lbs (3.5 kg)
Dimensions: 4.7(W) x 6.2(H) x 9.1(D) inches (119 x 158 x 232 mm)
Power Source: 12VDC, PoE+ (IEEE802.3at, Class 4)
Power Consumption: 24W Max.
Operating Conditions: -40°C to 60°C (-40°F to 140°F)
Warranty: 5-year warranty